( TL19E00J18513415023KBAT00 )

Rear Bumper Finisher Cover Replacement

R20A3 Engine Model
NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the rear bumper and the body.

1. Remove the rear bumper.

1. Remove the screw and the clips (A). Pull the rear bumper finisher cover (B) away to release the grooves (C), then remove the cover from the rear bumper (D).

1. Install the cover in the reverse order of removal, and note these items:
   - If the clips are damaged, replace them with new ones.
   - Push the clips into place securely.