( TL19E1PE1041141228CKBAT00 )

A/T Shift Lever Boot and A/T Gear Position Indicator Panel Base Replacement

1. Install the A/T gear position indicator panel base (A) on the shift lever bracket (B).
   NOTE: Take care not to pinch the harness.

1. Install the A/T gear position indicator panel light socket (C) in the indicator panel base.

1. For LHD model: Route the A/T gear position indicator panel light harness. Take a slack out of the harness, and secure the harness with at the guide.

1. Install the shift lever knob.

1. Install the shift lever assembly.