( TL19E00K70900081610FAAT00 )

DTC Troubleshooting: 61

1. Check for voltage between the ACC unit 20P connector No. 17 terminal and body ground.

Is there battery voltage?

YES | - | Repair an open in the wire between the ACC unit and the millimeter wave radar.■
NO | - | Check for loose or poor connections. If the connections are OK, update the ACC unit, then recheck. If the ACC unit was already updated, replace the ACC unit, then go to Step 18 .

1. Turn the ignition switch to LOCK (0).