( TL19E00J26273457073KDAT00 )

Steering Column Cover Removal/Installation

NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch or damage the column covers.
- Do not pry the cover surface with any tools.

1. Adjust the steering column to full tilt down position and to the full telescopic pull position.

1. Detach the clips fastening the column blind cover (A) from the upper column cover (B) by hand, and pull the pins (C) off the upper column cover.