( TL19E00F00000057101KDAT00 )

Steering Column Removal and Installation

SRS components are located in this area. Review the SRS component locations, and the precautions and procedures before doing repairs or service.
Removal

1. Adjust the steering column to full tilt down position, and to the full telescopic out position.

1. Do the battery terminal disconnection procedure.

1. Remove the driver's airbag and the steering wheel.

1. Remove the driver's dashboard undercover.

1. Remove the column covers.

1. Remove the steering joint cover (A).