( TL19E1AE34116317031KBAT00 )

Clutch Master Cylinder Replacement

NOTE:

- Use fender covers to avoid damaging painted surfaces.
- Do not spill brake fluid on the vehicle; it may damage the paint or plastic. If brake fluid does contact the paint or plastic, wash it off immediately with water.
- The illustrations show LHD model except where the procedure is defferent for RHD model.

1. Remove the brake fluid from the clutch master cylinder reservoir with a syringe or other suitable device.

1. Remove the clutch master cylinder reservoir (A).

LHD model
RHD model