( TL19E00J54200000000BBAT00 )

How to Troubleshoot the Body Electrical

HDS Inputs and Commands
Input:

System Menu | Data List | Data List Indication
--- | --- | ---
Lighting | Passing Input Signal | OFF/ON
Headlight ON Input Signal | OFF/ON
Driver's Door Switch | OFF/ON
Hazard Switch | OFF/ON
Headlight Switch (OFF) | OFF/ON
Headlight Switch (PARKING) | OFF/ON
Headlight Switch (HEADLIGHT) | OFF/ON
Headlight Switch (AUTO) | OFF/ON
Headlight Switch (High Beam) | OFF/ON
Headlight Switch (PASSING) | OFF/ON
Turn Signal Switch (LEFT) | OFF/ON
Turn Signal Switch (RIGHT) | OFF/ON
Fog Light Switch | OFF/ON
Rear Fog Light Switch | OFF/ON
Interior Light Command | OFF/ON
Left Turn Signal Command | OFF/ON
Right Turn Signal Command | OFF/ON
Rear Fog Light Command | OFF/ON
DR Courtesy Light Output | OFF/ON
RD Courtesy Light Output | OFF/ON
Headlight Command | OFF/ON
Headlight High Beam Command | OFF/ON
Parking Light Command | OFF/ON
Fog Light Command | OFF/ON
Autolight Sensor Input Voltage | V
Autolight Sensor Malfunction Detection Voltage Max | V
Autolight Sensor Malfunction Detection Voltage Min | V
Headlight Cleaner Command | OFF/ON
Autolight Small Command | OFF/ON
Autolight Headlight Command | OFF/ON
Autolight Warning Command | OFF/ON
Autolight Headlight Backup Line Command | OFF/ON
AS Courtesy Light Output | OFF/ON
RA Courtesy Light Output | OFF/ON