( TL19E00G10110249112FAAT00 )

Radiator and A/C Condenser Fan Low Speed Circuit Troubleshooting

1. Measure the voltage between the radiator fan 2P connector No. 2 terminal and body ground.

Is there battery voltage?

YES | - | Go to Step 19 .
NO | - | Repair open in the wire between the radiator fan relay and the radiator fan.■

1. Set the A/C button and fan control button OFF, then turn the ignition switch to LOCK (0).

1. Reconnect the radiator fan 2P connector.