( TL19E00J54226561997DCAT00 )

Under-dash Fuse/Relay Box (Passenger's) Connector Locations

Passenger's Under-dash Fuse/Relay Box

Socket | Ref | Terminal | Connects to | Notes
--- | --- | --- | --- | ---
A | 1 | 38 | Dashboard wire harness |
B | 8 | 1 | Dashboard wire harness |
|  |  | [Left engine compartment wire harness] |
C | 7 | 12 | Dashboard wire harness * |
D | 2 | 28 | Audio wire harness |
E | 6 | 18 | Right [left] engine compartment wire harness |
F | 5 | 2 | Right [left] engine compartment wire harness |
G | 3 | 16 | Not used |
H | 4 | 38 | Right [left] side wire harness |

[ ]: | RHD model

*: | With headlight washer