( TL19E00E16226622502KBAT00 )

Driveshaft Dynamic Damper Replacement

1. Remove the inboard joint.

1. Remove the dynamic damper band.

1. Remove the dynamic damper (A).

1. Install the new dynamic damper.
   NOTE: Be careful not to swap the dynamic dampers. Check the type of dynamic damper at its shape.

   Model | Left/Right Driveshaft | Dynamic Damper (A) Type
   --- | --- | ---
   R20A3 engine model | M/T | Left | 2
   Right | 1
   A/T | Left | 1
   Right | 1
   K24Z3 engine model | M/T | Left | 2
   Right | 1
   A/T | Left | 1
   Right | 2

Dynamic damper type 1
Dynamic damper type 2