( TL19E00R11100000000YCAT08 )

Front Body Construction

NOTE: Confirm that the sold as repair parts, refer to the appropriate Parts Catalog.
NOTE:

- The part marked with numbers are sold as repair parts.
- The part marked with letters are not sold separately and are shown only for reference.
- [ ]: Thickness unit: mm (in.)
- High-tension steel sheet: Tensioner strength 340 to 590 MPa.

No. | Part Name | Tensioner Strength (MPa) | Zinc-plating
--- | --- | --- | ---
(1) | Hood | Skin [0.7 (0.028)] | 340 | ○
Frame [0.55 (0.022)] | 270 | ○
(2) | Front Fender [0.75 (0.0295)] | 270 | ○
(3) | Front Bulkhead Comp.
-1 | Front Bulkhead Side Stay Set [0.7 (0.028)] | 270 | ○
-2 | Front Bulkhead Upper Frame Set |  |
a: | Bulkhead Upper Center Frame [0.8 (0.031)] | 270 | ○
b: | Bulkhead Upper Side Frame [1.0 (0.039)] | 270 | ○
c: | Bulkhead Side Stay Plate [0.6 (0.024)] | 270 | ○
-3 | Front Fender Front Bracket [1.0 (0.039)] | 270 | ○
-4 | Front Bulkhead Lower Cross-member Set [0.8 (0.031)] | 270 | ○
(4) | Front Wheelhouse Comp.
| a: | Front Damper Housing Upper [2.3 (0.091)]/Damper Base [2.0 (0.079)] | 270/440 | ○
b: | Front Damper Housing Lower [1.4 (0.055)] | 270 | ○
c: | Front Damper Housing Lower Extension [1.0 (0.039)] | 270 | ○
-1 | Front Wheelhouse Sub Set |  |
d: | Front Wheelhouse [0.7 (0.028)] | 270 | ○
e: | Front Wheelhouse Gusset [1.0 (0.039)] | 590 | ○
-2 | Front Wheelhouse Upper Inner Set |  |
f: | Front Wheelhouse Upper Inner [1.0 (0.039)] | 590 | ○
-3 | Front Fender Middle Bracket [1.0 (0.039)] | 270 | ○
-4 | Front Wheelhouse Lower Member [0.6 (0.024)] | 590 | ○
(5) | Front Wheelhouse Upper Member Comp.
| a: | Front Wheelhouse Upper Member [0.7 (0.028)] | 590 | ○
b: | Front Wheelhouse Upper Member Bulkhead [1.0 (0.039)] | 270 | ○
c: | Front Wheelhouse Lower Member Extension [0.6 (0.024)] | 590 | ○
(6) | Front Side Frame Comp.
| a: | Front Side Frame Front [1.6 (0.063)], Rear [1.8 (0.071)] | 590 | ○
b: | Front Side Backplate Front [1.4 (0.055)], Rear [1.8 (0.071)] | 590 | ○
c: | Side Frame Rear End [2.0 (0.079)]/Outrigger [1.4 (0.055)] | 590 | ○
-1 | Front Lower Member Support Set [0.6 (0.024)] | 590 | ○
-2 | Front Subframe Support Bracket Set [1.6 (0.063)] | 590 | ○
-3 | Bumper Beame Side Bracket [2.3 (0.091)] | 590 | ○
(7) | Dashboard Upper Comp.
| a: | Dashboard Upper [0.7 (0.028)] | 270 | ○
b: | Dashboard Upper Cross-member [0.7 (0.028)] | 270 |
c: | Dashboard Upper Side Member [1.8 (0.071)] | 440 | ○
-1 | Front Fender Rear Bracket [0.8 (0.031)] | 270 | ○
(8) | Dashboard Lower | Upper [0.9 (0.035)] | 270 | ○
Lower [1.2 (0.047)] | 590 | ○