( TL19E00K791000R8561FAAT00 )

DTC Troubleshooting: 85-61, 85-62

1. Measure the resistance between No. 1 terminal of SRS unit connector B (39P) and body ground. There should be 1 MΩ.

Is the resistance as specified?

YES | - | Go to Step 12 .
NO | - | Short to ground between the No. 1 terminal of the SRS unit connector B (39P) and the No. 7 terminal of the OPDS unit harness 18P connector (dashboard wire harness, right side wire harness, SRS floor wire harness, or OPDS unit harness); replace the faulty harness.■