( TL19E00J26220219281KDAT00 )

Dashboard Center Lower Cover Removal/Installation

SRS components are located in this area. Review the SRS component locations and the precautions and procedures before doing repairs or service.
NOTE:

- Take care not to scratch the dashboard and its related parts.
- When removing components, use the trim tools or equivalent.
- LHD model is shown; RHD model is symmetrical.

1. Remove the center console panel.

1. Detach the clips (A, B, C) by pulling the front edges of the center console (D) out from both sides, then release both front portions of the console from the dashboard as needed.