( TL19E00D14300014781LCAT00 )

Brake Master Cylinder Disassembly

NOTE: The illustrations show LHD model.

1. Remove the master cylinder.

1. Remove the rod seal from the master cylinder.

1. Remove the circlip (A) while pushing in the secondary piston (B).

1. Remove the reservoir (A).

1. Remove the stop pin (B) while pushing in the secondary piston (C).

1. Remove the piston guide (A), secondary piston (B) and primary piston (C).

1. Remove the reservoir seal (A) from the reservoir cap (B).

1. Remove the strainer (C) and grommets (D) from the reservoir (E).
   NOTE: When reservoir and master cylinder body are separated, replace the grommets with new ones.