( TL19E00D14300014801MBAT00 )

Brake Pedal and Brake Pedal Position Switch Adjustment

Pedal Free Play

1. With the ignition switch in LOCK (0), inspect the play (A) at the brake pedal pad (B) by pushing the brake pedal by hand. If the brake pedal free play is out of specification, adjust the brake pedal position switch (C). If the brake pedal free play is insufficient, it may result in brake drag.

   Free play: | 1−5 mm (0.04−0.20 in.)