( TL19E00K70900081620FAAT00 )

DTC Troubleshooting: 62

DTC 62:
Millimeter Wave Radar Sensor Error

1. Clear the DTCs with the HDS.

1. Turn the ignition switch to ON (II) and the main switch to ON.

1. Check for DTCs with the HDS.

Is DTC 62 indicated?

YES | - | Check for loose or poor connections. If the connectors are OK, replace the millimeter wave radar. After replacement, do the millimeter wave radar aiming. ■
NO | - | Intermittent failure, the system is OK at this time.■