( TL19E00H32500000000FAAT15 )

LKAS Symptom Troubleshooting - LKAS activation indicator (green) does not go off

LKAS activation indicator (green) does not go off

1. Do the gauge control module self-diagnostic function.

Is the gauge control module OK?

YES | - | Go to Step 2 .
NO | - | Substitute a known-good gauge control module and recheck. If the problem goes away, replace the original gauge control module. ■

1. Remove the ACC combination switch from the steering wheel. ■

1. Turn the ignition switch to ON (II).

1. Watch the LKAS activation indicator.

Does the LKAS activation indicator go off?

YES | - | Test the distance/LKAS switch. ■
NO | - | Repair a short to ground in the wire between the ACC combination switch and the gauge control module.■