( TL19E00J4612705366NKBAT00 )

Front Seat Slide Lever Replacement

Manual Height Adjustable Seat/Manual Seat
NOTE:

- Put on gloves to protect your hands.
- Take care not to tear the seams or damage the seat covers.

1. Remove the front seat.

1. Lift up the front seat, and pull the slide lever (A) out while prying up the spring (B) from the lever holders (C) of both seat tracks, then remove the lever.

1. Install the slide lever by pushing on it into the lever holders of both seat tracks until the springs snap the slits in the lever.

1. Apply multipurpose grease to the pivot portions of the slide locks.