( TL19E30A46500000000HBAT00 )

Starting System Symptom Troubleshooting Index

Symptom | Diagnostic procedure | Also check for
--- | --- | ---

Engine does not start (does not crank)

1.
2.
3.
4.
5.
6.

Check for loose battery terminals or connections.
Test the battery for a low state of charge.
Check the starter.
Check the starter cut relay.
Check the transmission range switch (A/T model).
Check the ignition switch or related circuits.

Poor ground at G101 (A/T model)

Engine cranks, but does not start

1.
2.
3.
4.
5.
6.
7.
8.

Check for PGM-FI DTCs.
Check the fuel pressure.
Check for a plugged or damaged fuel line.
Check for a plugged fuel filter.
Check the throttle body.
Check for low engine compression
Check for a damaged or broken cam chain.
Do the engine control module (ECM)/powertrain control module (PCM) reset function with the Honda Diagnostic System (HDS) to cancel the ALL INJECTORS STOP function.

Engine is hard to start | 1. 2. 3. 4. | Check for PGM-FI DTCs. Check the fuel pressure. Check for a plugged or damaged fuel line. Check for a plugged fuel filter. |
Engine cranks slowly | 1. 2. 3. 4. | Check for loose battery terminals or connections. Test the battery for a low state of charge. Check the starter for binding. Check for excessive drag in the engine. |