( TL19E00J46636200000FAAT04 )

Immobilizer System Symptom Troubleshooting - Immobilizer indicator does not go off

Immobilizer indicator does not go off

1. Turn the ignition switch to LOCK (0).

1. Connect the HDS to the data link connector.

1. Turn the ignition switch to ON (II).

1. Enter the IMMOBILIZER, then select the IMMOBILIZER INFORMATION.

1. Do the SYSTEM CHECK with the HDS.

Is N-1 OK indicated?

YES | - | Replace the gauge control module. ■
NO | - | Substitute a known-good immobilizer-keyless control unit , then register it and recheck. If the symptom goes away, replace the original immobilizer-keyless control unit. ■