( TL19E00J18513415017KBAT00 )

Front Bumper Lower Grille Replacement

1. Remove the induction center plate (A) from the front bumper (B).

   -1. | With headlight washer: Release the washer tube (C) from the holders (D) of the plate.
   -2. | Remove the clips from under the bumper.
   -3. | Remove the screws.
   -4. | Pull the plate out to detach the hooks (E). NOTE: To remove the clips, pry the inner clip up at the edge near the line (F) on its head.