( TL19E00J54300065041KBAT00 )

Washer Tube Replacement

1. Remove the right front inner fender.

1. Remove the washer nozzles and clips, then remove the tubes.

1. Install the parts in the reverse order of removal. Take care not to pinch the washer tubes. Check the washer operation.

With Headlight Washer

1. Remove the right front inner fender.

1. Remove the washer nozzles and clips, then remove the tubes.

With Headlight Washer

1. Install the parts in the reverse order of removal. Take care not to pinch the washer tubes. Check the washer operation.