( TL19E1PE10400000000HAAT35 )

Shift lever does not operate smoothly

Probable Cause(s)

1. Transmission range switch defective or out of adjustment
2. Shift cable broken or out of adjustment
3. Connection between shift cable and transmission or body is worn

Notes

- Check for a stored DTC, and check for loose connectors.
- Inspect the transmission range switch for operation.
- Check for a loose shift cable at the shift lever and the transmission control shaft.