( TL19E00B44100036401KBAT00 )

Rear Knuckle/Hub Bearing Unit Replacement

Exploded View-Rear Disc Brake Type
Exploded View-Rear Drum In Disc Brake Type
Special Tools Required
Ball joint remover, 32 mm
07MAC-SL00101
NOTE: The illustrations show only the rear disc brake type of the vehicle except where the procedure is different for the rear drum in disc brake type.
Hub Bearing Unit Replacement

1. Raise the rear of the vehicle, and support it with safety stands in the proper locations.

1. Remove the wheel nuts, and the rear wheel.

1. Release the parking brake lever fully.

1. Rear disc brake type: Loosen the parking brake cable adjusting nut.