( TL19E00J26273413801KDAT00 )

Interior Trim Removal/Installation - Pillar Areas

Rear Pillar Trim
SRS components are located in this area. Review the SRS component locations and the precautions and procedures before doing repairs or service.
NOTE:

- Follow the rear pillar trim installation procedure carefully; improper installation could cause the side curtain airbag to deploy improperly and possibly cause injury.
- Put on gloves to protect your hands.
- When removing components, use the trim tools or equivalent.
- Take care not to scratch the trim and the panels.
- The upper clip in the rear pillar trim (A) consists of a resin grommet (B) and a metal pin (C). The grommet expanded with the pin secures it to the body panel (D). The grommet must be replaced with a new one when the trim is reinstalled.