( TL19E00J46127053676KBAT00 )

Front Seat Frame Replacement

Passenger's Seat
NOTE:

- Put on gloves to protect your hands.
- When removing components, use the trim tools or equivalent.
- If the side airbag has deployed, replace the seat frame and related parts with new ones.
- LHD model is shown; RHD model is symmetrical.

1. Remove the front seat.

1. Remove these items:
   - Front seat-back cover/pad
   - Front seat cushion cover/pad
   - OPDS unit (for some models)
   - Seat belt buckle
   - Side airbag

1. Remove the recline inner cover (A) and the center inner cover (B) from the seat frame (C).

1. Install the new seat frame in the reverse order of removal.

8-way power seat
Manual seat