( TL19E00J46127053949KBAT00 )

Front Seat-back Cover Replacement

SRS components are located in this area. Review the SRS component locations and the precautions and procedures before doing repairs or service.
NOTE:

- Put on gloves to protect your hands.
- Take care not to tear the seams of damage the seat covers.
- With OPDS: On the passenger's seat, do not touch the OPDS sensor in the seat-back pad, and keep it away from oil. Oil can corrode the sensor causing it to fail.
- When removing components, use the trim tools or equivalent.
- LHD model is shown; RHD model is symmetrical.

1. Remove the front seat.

1. Driver's seat: Remove the clip (A), then remove the lumbar support handle (B).