( TL19E00D00060814731MAAT00 )

Parking Brake Inspection

1. Measure the inside diameter of the parking brake drum with inside vernier calipers.

   Parking brake drum inside diameter:
   | Standard: | 189.9−190.0 mm (7.476−7.480 in.)
   | Service limit: | 191.0 mm (7.520 in.)

1. If the inside diameter of the parking brake drum is more than service limit, replace the brake disc/drum.

1. Check the parking brake disc/drum for scoring, grooves, and cracks.

1. Clean the mating surface of the brake disc/drum and the inside of the wheel, then install the rear wheels.