( TL19E00J46636234525MBAT00 )

Immobilizer-Keyless Control Unit Registration

1. Turn the ignition switch to ON (II).

1. Connect the HDS to the data link connector (DLC).

1. Select IMMOBILIZER from the SYSTEM SELECT MENU.

1. Select the IMMOBILIZER SETUP from the MODE menu, then select the REPLACE IMM UNIT from the IMMOBILIZER MENU.

1. Do the registration according to the instruction of the HDS screen.

1. Check if the engine can be started by the registered immobilizer-keyless control unit.