( TL19E00K75100081230FAAT00 )

DTC Troubleshooting: 23

LKAS Control Unit DTC 23:
Gauge Control Module Malfunction

1. Clear the DTCs with the HDS.

1. Turn the ignition switch to LOCK (0), then turn it to ON (II).

1. Check for LKAS control unit DTCs with HDS.

Is DTC 23 indicated?

YES | - | Check for the gauge control module DTCs, then troubleshoot the indicated DTC.■
NO | - | Intermittent failure, the system is OK at this time.■