( TL19E00K773000Y1828FAAT00 )

DTC Troubleshooting: B1828

1. Check for continuity between body ground and recline motor/position sensor 5P connector No. 1 and No. 2 terminals individually.

Is there continuity?

YES | - | Repair a short to ground in the wire.■
NO | - | Go to Step 31 .

1. Test the recline motor.

Is the motor OK?

YES | - | Replace the power seat control unit .■
NO | - | Replace the recline motor/position sensor.■