( TL19E1PE1041074485AFAAT00 )

A/T Paddle Shifter + (Upshift Switch) Illumination Circuit Troubleshooting

SRS components are located in this area. Review the SRS component locations and the precautions and procedures in the SRS before doing repair or service.

1. Remove the steering wheel.

1. Check for continuity between cable reel subharness 20P connector terminals No. 3 and No. 4.

Is there continuity?

YES | - | Go to Step 5 .
NO | - | Go to Step 3 .

1. Disconnect the paddle shifter + (upshift switch) connector.