( TL19E00K764000Y1149FAAT00 )

DTC Troubleshooting: B1149

DTC B1149:
Right Rear Power Window Position Information Error

1. Clear the DTC with the HDS.

1. Turn the ignition switch to LOCK (0) and then back to ON (II).

1. Open and close the right rear power window by using the right rear power window switch manually.

1. Check for DTCs with the HDS.

Is DTC B1149 indicated?

YES | - | Go to Step 5 .
NO | - | Intermittent failure, the system is OK at this time. Check for loose or poor connections.■

1. Check for DTCs with the HDS.

Is DTC B1134 and B1135 indicated?

YES | - | Troubleshoot the indicated DTC(s) first.■
NO | - | Reset the right rear power window, and recheck.