( TL19E1AE34150339091MFAT00 )

M/T Change Lever Assembly Disassembly/Reassembly

NOTE:

- Do not install components if too much time has passed after applying liquid gasket. Instead, remove the old residue and reapply the liquid gasket.
- Prior to reassembling, clean all parts in solvent, dry them, and apply grease to the contact surfaces as shown.

NOTE:

- Do not install components if too much time has passed after applying liquid gasket. Instead, remove the old residue and reapply the liquid gasket.
- Prior to reassembling, clean all parts in solvent, dry them, and apply grease to the contact surfaces as shown.