( TL19E00B54100000000BAAT00 )

The Extraction of the Fluid Sealant of the Tyre Inflator

1. Use the empty bottle (A) to extract the fluid sealant. Insert the tube into the tyre through the drain hole, and stick it down until the end of the tube is immersed into the fluid sealant (B).

1. Set the empty bottle in the lower position than the tyre and pump the fluid sealant into the bottle. To empty the tyre, pump it completely by shaking the tyre or doing something else.