( TL19E00H15300000000CAAT00 )

CMBS operation

- Warnings are both audible (warning buzzer) and visual (MID)
- Evasive action support and collision-speed reduction by brake control

(1) Approaching a vehicle ahead:
The CMBS warns the driver by a MID indication and buzzer sound.

(2) Closer to vehicle ahead:

- Warning by a MID indication and buzzer sound.
- CMBS aids perception and evasive action by using the sensory warning of light braking.

(3) Collision unavoidable:

- Warnings by a MID indication and buzzer sound.
- CMBS reduces collision speed to minigate damage.