( TL19E00J46636200000FAAT02 )

Immobilizer System Symptom Troubleshooting - Engine does not start with the immobilizer key

Engine does not start with the immobilizer key
NOTE: Before troubleshooting, check the items listed in ‘‘General Check before Troubleshooting''.

1. Try to start the engine.

Does the engine start?

YES | - | Intermittent failure, the vehicle is OK at this time.■
NO | - | Go to Step 2 .

1. Turn the ignition switch to LOCK (0).

1. Turn the ignition switch to ON (II), and check the immobilizer indicator.

Does the indicator cone on for 2 seconds, then go off?

YES | - | Go to Step 4 .
NO | - | Go to the immobilizer indicator blinks troubleshooting. ■

1. Turn the ignition switch to START (III).

Does the starter motor run?

YES | - | Go to Step 5 .
NO | - | Go to Starting System, and check the starter motor. ■

1. Try to start the engine with the immobilizer key.

Does the engine start?

YES | - | Go to Step 6 .
NO | - | Go to the PGM-FI System Symptom Troubleshooting. ■

1. Wait for a few minutes with the engine running.

Does the engine stop?

YES | - | Go to the PGM-FI System Symptom Troubleshooting. ■
NO | - | The system is OK at this time.■