( TL19E3AA14500000000HAAT10 )

Set speed will not resume when the resume/accel switch is pressed (with the cruise control main switch turned on, and set speed temporarily canceled by pressing the clutch pedal)

Diagnostic procedure

1. Check for PGM-FI DTCs.
2. Check the clutch pedal position switch adjustment.
3. Do the cruise control combination switch test.
4. Do the cruise control input test. Test the resume/accel switch signal input. Test the clutch pedal position switch signal input.

Also check for

- Faulty clutch pedal position switch
- Open circuit, loose or disconnected terminals: LT BLU, GRY wire