( TL19E00J26216516409KDAT00 )

Center Console Panel Removal/Installation

NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the front seat, the dashboard, and the related parts.
- When removing components, use the trim tools or equivalent.
- LHD model is shown; RHD model is symmetrical.

1. M/T model except Type-S: Lower the shift lever boot (A) to release the hooks (B) from the boot, then remove the shift knob (C).