( TL19E00D00060814811KBAT00 )

Parking Brake Shoe Replacement

1. Clean the threaded portions of the clevis A, and coat the threads of the clevis with grease. Clean the sliding surface of the clevis B, and coat the sliding surface of the clevis B with grease. Install the clevis A and B on the adjuster (C) and shorten the clevis A by turning the adjuster.

1. Position the brake shoe adjuster assembly (D) on the parking brake shoes.

1. Reinstall the upper return spring (E).

1. Install the rear brake disc/drum and the rear brake caliper.

1. Do the major parking brake adjustment.