( TL19E00H15300000000CAAT00 )

Main functions of CMBS

- When a collision with a vehicle ahead is about to happen at a vehicle speed more than 15 km/h (9 mph) and the relative speed (the speed difference from the vehicle ahead) is more than 15 km/h (9 mph), the system provides warnings (audible and visual) and brake control.
- When approaching a vehicle ahead and the distance to the vehicle ahead is very close, the system provides the collision warning (1st stage) by the MID indication and buzzer sound.
- When the closing distance continues to decrease and there is a high risk of collision, the system applies light braking (2nd stage) with the 1st stage warning.
- When the system judges that a collision is imminent, the system activates emergency brake control.