( TL19E1PE10410434083KBAT00 )

A/T End Cover Idler Gear Shaft Bearing Replacement

Special Tools Required
Adjustable bearing remover set
07JAC-PH80000
Driver handle 15 x 135L
07749-0010000
Bearing driver attachment 52 x 55 mm
07746-0010400

1. Remove the idler gear shaft bearing (A) from the end cover (B) using the adjustable bearing remover set.

1. Install a new bearing in the end cover using the 15 x 135L driver handle and the 52 x 55 mm bearing driver attachment.