( TL19E00K722000R3401FAAT00 )

DTC Troubleshooting: 34-01

DTC 34-01:
Power Relay Stuck ON (Ignition Switch is in LOCK (0))

1. Turn the ignition switch to ON (II).

1. Clear the DTC with the HDS.

1. Turn the ignition switch to LOCK (0).

1. Turn the ignition switch to ON (II).

1. Check for DTCs with the HDS.

Is DTC 34-01 indicated?

YES | - | Replace the EPS control unit. ■
NO | - | Intermittent failure, the system is OK at this time.■