( TL19E1PE10410459801KCAT00 )

A/T Shaft Assembly and Housing Installation

1. Install a new O-ring (F) on the shift solenoid wire harness (G), then install the shift solenoid wire harness in the transmission housing. Secure the shift solenoid wire harness with the bolt (H).

1. Connect the shift solenoid wire harness terminals to the shift solenoid valves:
   - BLU wire connector to shift solenoid valve A.
   - ORN wire connector to shift solenoid valve B.
   - GRN wire connector to shift solenoid valve C.
   - YEL, WHT, and WHT wire connector to shift solenoid valve D.
   - RED wire connector to shift solenoid valve E.