( TL19E00J46166453632KBAT00 )

Rear Seat Cushion Cover Replacement

1. Install the cover in the reverse order of removal, and note these items:
   - To prevent wrinkles when installing a seat cushion cover, make sure the material is stretched evenly over the pad before securing the upholstery rings.
   - Replace any upholstery rings (A) you removed with new ones. Install them with commercially available upholstery ring pliers (B).