( TL19E00J46127053632KBAT00 )

Front Seat Cushion Cover Replacement

1. Install the cover in the reverse order of removal, and note these items:
   - To prevent wrinkles when installing a seat cushion cover, make sure the material is stretched evenly over the pad before securing the clips and hook strips.
   - Replace any upholstery rings you removed with new ones (A). Install them with commercially available upholstery ring pliers (B).