( TL19E00K791000R331XFAAT00 )

DTC Troubleshooting: 33-1x

1. Check for continuity between the No. 1 and the No. 2 terminals of SRS floor wire harness 2P connector.

Is there continuity?

YES | - | Faulty SRS unit or poor connection at SRS unit connector A (39P) and the SRS unit. Check the connection between the connector and the SRS unit. If the connection is OK, replace the SRS unit. ■
NO | - | Open in the SRS floor wire harness; replace the SRS floor wire harness.■