( TL19E00D14300014711LAAT10 )

Front Brake Caliper Overhaul

Disassembly - 2-piston caliper type

1. Remove the caliper body.

1. Mount the commercially available brake caliper piston compressor tool (A) on the caliper body (B) as shown. Blow out the pistons with compressed air gradually, and remove the pistons from the caliper body.
   NOTE: Do not put the hand into the caliper body. Because the piston might dash out mightily in the caliper body.