( TL19E00J10300000000FAAT05 )

Audio System Symptom Troubleshooting - No sound is heard from the speaker(s) (display is normal) (with premium audio system)

1. Measure the voltage between stereo amplifier connector A (18P) terminal No. 18 and body ground.

Is there battery voltage?

YES | - | Go to Step 16 .
NO | - | Repair open in the wire between No. 15 (20 A) fuse in the passenger's under-dash fuse/relay box and stereo amplifier connector B (18P) terminal No. 18.■

1. Disconnect stereo amplifier connector B (28P).

1. Turn the ignition switch to ON (II).