( TL19E00J46127053632KBAT00 )

Front Seat Cushion Cover Replacement

1. 8-way power seat: Remove the recline cover (A). The driver's seat is shown; the passenger's seat is symmetrical.

   -1. | Remove the screw, and detach the clip.
   -2. | Detach the tabs (B).
   -3. | Pull up the cover, then release the hook (C) and the tab (D).
   -4. | Disconnect the power seat adjustment switch connector (E).
   -5. | Detach the tabs (F), then remove the upper recline inner cover (G) from the recline cover.